{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":10,"n_cols":62,"rows_kept":10,"flags":["formulas_cached_only"]}
["卡片ID","报告卡编号","省份名称","市名称","区县名","行政区划代码","区县人口数","采样类型","水期类型","供水单位编号","供水单位名称","供水单位详细地点","供水方式","深度处理（臭氧活性炭、膜工艺等）","特殊处理（除氟、除砷、除铁、除锰等）","制水工艺：其他","检测类型","水源类型","水样类型","消毒方式","消毒设备使用情况","建成时间","正式运营时间","总投资","中央投资","供水覆盖人口","监测类型","设计供水能力","实际供水能力","供水工程解决的主要问题","取样日期","测定日期","监测点所在乡镇","监测点所在村","学校名称","学校类别","办学性质","学生总数","住宿学生人数","教职员工数","工程类型","卫生许可情况","采样乡镇（详细地址）","采样乡镇行政区划代码","监测项目","总大肠菌群（MPN/100mL或CFU/100mL）","耐热大肠菌群（MPN/100mL或CFU/101mL）","大肠埃希氏菌（MPN/100mL或CFU/102mL）","菌落总数（CFU/mL）","色度（铂钴色度单位）","浑浊度（NTU-散射浊度单位）","嗅和味","肉眼可见物","pH","氯化物（mg/L）","总硬度(以CaCO3计，mg/L）","耗氧量（CODMn法，以O2计，mg/L）","硝酸盐氮（以N计，mg/L）","砷（mg/L）","铬（六价，mg/L）","铁（mg/L）","锰（mg/L）"]
["29db34db-b8f8-4409-83b0-b4f6f6bcafa7","21070200201905167481\t","辽宁省","锦州市","古塔区",21070201,421346,"城市水","枯水期","210781002c","锦州市大穆水厂","凌海市松山乡大穆村","常规处理（含混凝、沉淀、过滤、消毒)","无","无",null,"常规指标和氨氮","深井","末梢水","液氯","按要求使用",{"$nulls":4},480000,6,200000,160000,null,"2020-08-18","2020-08-18","不详乡镇","松山乡",{"$nulls":7},"有卫生许可","站前街道，城北阳光",21070201,"-",0,null,null,42,"<5","<0.5",0,0,7.45,99.3,365.5,1.36,3.7,"<0.001","<0.004","<0.10","<0.05"]
["6683d193-bd7c-47ca-a7ca-28a83f2081a6","21070200201905167144\t","辽宁省","锦州市","古塔区",21070204,421346,"城市水","枯水期","210781002c","锦州市大穆水厂","凌海市松山乡大穆村","常规处理（含混凝、沉淀、过滤、消毒)","无","无",null,"常规指标和氨氮","深井","末梢水","液氯","按要求使用",{"$nulls":4},480000,6,200000,160000,null,"2020-08-19","2020-08-19","不详乡镇","松山乡",{"$nulls":7},"有卫生许可","北街街道，阜康",21070204,"-",0,null,null,120,"<5","<0.5",0,0,7.94,132.3,461.7,1.01,4.4,"<0.001","<0.004","<0.10","<0.05"]
["9a05e14e-6c95-42a0-b484-afb951abf868","21070200201905166991\t","辽宁省","锦州市","古塔区",21070209,421346,"城市水","枯水期","210781002c","锦州市大穆水厂","凌海市松山乡大穆村","常规处理（含混凝、沉淀、过滤、消毒)","无","无",null,"常规指标和氨氮","深井","末梢水","液氯","按要求使用",{"$nulls":4},480000,6,200000,160000,null,"2020-08-18","2020-08-18","不详乡镇","松山乡",{"$nulls":7},"有卫生许可","士英街道，市疾控中心",21070209,"-",0,null,null,32,"<5","<0.5",0,0,7.35,44.5,201.6,1.82,0.3,"<0.001","<0.004","<0.10","<0.05"]
["fa27fd13-eb7b-4534-80f0-bc541afdeb91","21071100201905164592\t","辽宁省","锦州市","太和区",21071101,151782,"城市水","枯水期","210781002c","锦州市大穆水厂","凌海市松山乡大穆村","常规处理（含混凝、沉淀、过滤、消毒)","无","无",null,"常规指标和氨氮","深井","末梢水","液氯","按要求使用",{"$nulls":4},480000,6,200000,160000,null,"2020-08-19","2020-08-19","不详乡镇","松山乡",{"$nulls":7},"有卫生许可","凌西街道，石化新区",21071101,"-",0,null,null,120,"<5","<0.5",0,0,7.62,73.4,271.8,2.74,1.6,"<0.001","<0.004","<0.10","<0.05"]
["63bbeaa0-6d12-4460-9f5d-1b87ce92dc4b","21071100201905164725\t","辽宁省","锦州市","太和区",21071113,151782,"城市水","枯水期","210781002c","锦州市大穆水厂","凌海市松山乡大穆村","常规处理（含混凝、沉淀、过滤、消毒)","无","无",null,"常规指标和氨氮","深井","末梢水","液氯","按要求使用",{"$nulls":4},480000,6,200000,160000,null,"2020-08-18","2020-08-18","不详乡镇","松山乡",{"$nulls":7},"有卫生许可","松山街道，富锦佳园",21071113,"-",0,null,null,100,"<5",0.6,0,0,7.45,138.6,393.9,1.08,4.4,"<0.001","<0.004","<0.10","<0.05"]
["dd7a6f56-d6e0-436a-aef4-c9646813a5e9","21071100201905163870\t","辽宁省","锦州市","太和区",21071114,151782,"城市水","枯水期","210781002c","锦州市大穆水厂","凌海市松山乡大穆村","常规处理（含混凝、沉淀、过滤、消毒)","无","无",null,"常规指标和氨氮","深井","末梢水","液氯","按要求使用",{"$nulls":4},480000,6,200000,160000,null,"2020-08-18","2020-08-18","不详乡镇","松山乡",{"$nulls":7},"有卫生许可","果树农场街道，大蟹天下",21071114,"-",0,null,null,120,"<5",0.7,0,0,7.65,146.1,470.9,0.94,4.6,"<0.001","<0.004","<0.10","<0.05"]
["23a88df4-45da-48ab-bbcb-621c645c8572","21071100201905163788\t","辽宁省","锦州市","太和区",21071114,151782,"城市水","枯水期","210781002c","锦州市大穆水厂","凌海市松山乡大穆村","常规处理（含混凝、沉淀、过滤、消毒)","无","无",null,"常规指标和氨氮","深井","末梢水","液氯","按要求使用",{"$nulls":4},480000,6,200000,160000,null,"2020-08-19","2020-08-19","不详乡镇","松山乡",{"$nulls":7},"有卫生许可","果树农场街道，尚海雅居",21071114,"-",0,null,null,92,"<5",0.6,0,0,7.74,139.7,{"v":496,"d":"496.0"},1.32,4.4,"<0.001","<0.004","<0.10","<0.05"]
["ca973e71-aeca-4965-aaf4-0f284b935e72","21071100201905165014\t","辽宁省","锦州市","太和区",21071115,151782,"城市水","枯水期","210781002c","锦州市大穆水厂","凌海市松山乡大穆村","常规处理（含混凝、沉淀、过滤、消毒)","无","无",null,"常规指标和氨氮","深井","末梢水","液氯","按要求使用",{"$nulls":4},480000,6,200000,160000,null,"2020-08-19","2020-08-19","不详乡镇","松山乡",{"$nulls":7},"有卫生许可","松山街道，曼哈顿",21071115,"-",0,null,null,50,"<5","<0.5",0,0,7.33,136.7,404.8,0.85,4.5,"<0.001","<0.004","<0.10","<0.05"]
["912bd237-0fc5-41a0-8d50-f7782964e7ac","21071100201905165579\t","辽宁省","锦州市","太和区",21071116,151782,"城市水","枯水期","210781002c","锦州市大穆水厂","凌海市松山乡大穆村","常规处理（含混凝、沉淀、过滤、消毒)","无","无",null,"常规指标和氨氮","深井","末梢水","液氯","按要求使用",{"$nulls":4},480000,6,200000,160000,null,"2020-08-19","2020-08-19","不详乡镇","松山乡",{"$nulls":7},"有卫生许可","巧鸟街道，海岸江南",21071116,"-",0,null,null,96,"<5",0.5,0,0,7.65,132.2,472.5,1.12,4.2,"<0.001","<0.004","<0.10","<0.05"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}