{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":7,"n_cols":62,"rows_kept":7,"flags":["formulas_cached_only"]}
["卡片ID","报告卡编号","省份名称","市名称","区县名","行政区划代码","区县人口数","采样类型","水期类型","供水单位编号","供水单位名称","供水单位详细地点","供水方式","深度处理（臭氧活性炭、膜工艺等）","特殊处理（除氟、除砷、除铁、除锰等）","制水工艺：其他","检测类型","水源类型","水样类型","消毒方式","消毒设备使用情况","建成时间","正式运营时间","总投资","中央投资","供水覆盖人口","监测类型","设计供水能力","实际供水能力","供水工程解决的主要问题","取样日期","测定日期","监测点所在乡镇","监测点所在村","学校名称","学校类别","办学性质","学生总数","住宿学生人数","教职员工数","工程类型","卫生许可情况","采样乡镇（详细地址）","采样乡镇行政区划代码","监测项目","总大肠菌群（MPN/100mL或CFU/100mL）","耐热大肠菌群（MPN/100mL或CFU/101mL）","大肠埃希氏菌（MPN/100mL或CFU/102mL）","菌落总数（CFU/mL）","色度（铂钴色度单位）","浑浊度（NTU-散射浊度单位）","嗅和味","肉眼可见物","pH","氯化物（mg/L）","总硬度(以CaCO3计，mg/L）","耗氧量（CODMn法，以O2计，mg/L）","硝酸盐氮（以N计，mg/L）","砷（mg/L）","铬（六价，mg/L）","铁（mg/L）","锰（mg/L）"]
["fa27fd13-eb7b-4534-80f0-bc541afdeb91","21071100201905164592\t","辽宁省","锦州市","太和区",21071101,151782,"城市水","枯水期","210781002c","锦州市大穆水厂","凌海市松山乡大穆村","常规处理（含混凝、沉淀、过滤、消毒)","无","无",null,"常规指标和氨氮","深井","末梢水","液氯","按要求使用",{"$nulls":4},480000,6,200000,160000,null,"2019-04-10","2019-04-10","不详乡镇","松山乡",{"$nulls":7},"有卫生许可","凌西街道，石化新区",21071101,"-",0,null,null,7,2.5,0.25,0,0,7.22,151.4,443.7,0.6,4,0.0005,0.002,0.05,0.025]
["63bbeaa0-6d12-4460-9f5d-1b87ce92dc4b","21071100201905164725\t","辽宁省","锦州市","太和区",21071113,151782,"城市水","枯水期","210781002c","锦州市大穆水厂","凌海市松山乡大穆村","常规处理（含混凝、沉淀、过滤、消毒)","无","无",null,"常规指标和氨氮","深井","末梢水","液氯","按要求使用",{"$nulls":4},480000,6,200000,160000,null,"2019-04-09","2019-04-09","不详乡镇","松山乡",{"$nulls":7},"有卫生许可","松山街道，富锦佳园",21071113,"-",0,null,null,9,2.5,0.25,0,0,7.28,139.5,406.5,0.65,3.9,0.0005,0.002,0.05,0.025]
["dd7a6f56-d6e0-436a-aef4-c9646813a5e9","21071100201905163870\t","辽宁省","锦州市","太和区",21071114,151782,"城市水","枯水期","210781002c","锦州市大穆水厂","凌海市松山乡大穆村","常规处理（含混凝、沉淀、过滤、消毒)","无","无",null,"常规指标和氨氮","深井","末梢水","液氯","按要求使用",{"$nulls":4},480000,6,200000,160000,null,"2019-04-11","2019-04-11","不详乡镇","松山乡",{"$nulls":7},"有卫生许可","果树农场街道，大蟹天下",21071114,"-",0,null,null,14,2.5,0.25,0,0,7.24,282.1,486.6,0.65,5,0.0005,0.002,0.05,0.025]
["23a88df4-45da-48ab-bbcb-621c645c8572","21071100201905163788\t","辽宁省","锦州市","太和区",21071114,151782,"城市水","枯水期","210781002c","锦州市大穆水厂","凌海市松山乡大穆村","常规处理（含混凝、沉淀、过滤、消毒)","无","无",null,"常规指标和氨氮","深井","末梢水","液氯","按要求使用",{"$nulls":4},480000,6,200000,160000,null,"2019-04-11","2019-04-11","不详乡镇","松山乡",{"$nulls":7},"有卫生许可","果树农场街道，易盈精工",21071114,"-",0,null,null,6,2.5,0.25,0,0,7.16,202.6,469.8,0.98,5.6,0.0005,0.002,0.05,0.025]
["ca973e71-aeca-4965-aaf4-0f284b935e72","21071100201905165014\t","辽宁省","锦州市","太和区",21071115,151782,"城市水","枯水期","210781002c","锦州市大穆水厂","凌海市松山乡大穆村","常规处理（含混凝、沉淀、过滤、消毒)","无","无",null,"常规指标和氨氮","深井","末梢水","液氯","按要求使用",{"$nulls":4},480000,6,200000,160000,null,"2019-04-10","2019-04-10","不详乡镇","松山乡",{"$nulls":7},"有卫生许可","松山街道，曼哈顿",21071115,"-",0,null,null,11,2.5,0.25,0,0,7.2,156,444.7,0.68,4,0.0005,0.002,0.05,0.025]
["912bd237-0fc5-41a0-8d50-f7782964e7ac","21071100201905165579\t","辽宁省","锦州市","太和区",21071116,151782,"城市水","枯水期","210781002c","锦州市大穆水厂","凌海市松山乡大穆村","常规处理（含混凝、沉淀、过滤、消毒)","无","无",null,"常规指标和氨氮","深井","末梢水","液氯","按要求使用",{"$nulls":4},480000,6,200000,160000,null,"2019-04-11","2019-04-11","不详乡镇","松山乡",{"$nulls":7},"有卫生许可","巧鸟街道，海岸江南",21071116,"-",0,null,null,13,2.5,0.25,0,0,7.19,290.7,514.6,0.63,5.4,0.0005,0.002,0.05,0.025]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}